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USER MANUAL
1. INTRODUCTION

Thank you for choosing the Acue Lighting Fusion 7 FX. To use this product correctly and safely, please read the instructions carefully before installing and using this product. This manual contains important installation and operation information. Make sure to strictly follow the instructions when installing and operating this product. Retain this manual in a safe place for future reference. 

The Fusion 7 FX uses a high-temperature resistant aluminum/metal body with hard plastic covers and is IP19 rated. IP19 is a classification given to devices that are designed mostly for indoor use in cool dry areas. This product is designed and produced in strict accordance with CE standards and conforms to the international standard of DMX512 signal protocol. It can be controlled manually from the display or by DMX using the built in 3-pin XLR in/out connectors. This fixture is suitable for various types of indoor concerts, indoor events, indoor installations, and other like environments.
2. SAFETY INSTRUCTIONS

· Please keep this User Manual for future reference. All users of this fixture must read the user manual thoroughly.

· Unpack and check contents carefully to make sure there is no damage caused by shipping before using the unit.

· Before operating, ensure that the voltage and frequency of power supply match the power requirements of the unit.

· It’s important to properly ground the fixture to avoid electric shock.

· The unit is designed for indoor use. It is alright to use outdoors temporarily but not when moisture is present. Do not point fixture directly into sunlight. Make sure main power connector is connected to an outlet that is not near liquids or moisture.
· The unit must be installed in a location with adequate ventilation, at least 50cm from adjacent surfaces. Be sure that no ventilation slots are blocked.

· Disconnect main power before moving fixture.

· Make sure there are no flammable materials close to the unit while operating, as it is fire hazard.

· Use safety cable when mounting this unit.
· Do not connect this product to power dimmers. 

· Max ambient operating temperature is 40˚C. Do not operate if the temperature is higher than this.

· Unit surface temperature may reach up to 85˚C. Do not touch the housing bare-handed during its operation. Turn off the power and allow about 15 minutes for the unit to cool down before replacing or serving.

· In the event of serious operating problem, stop using the unit immediately. Never try to repair the unit by yourself. Repairs carried out by unskilled individuals can lead to further damage or malfunction. Please contact the nearest authorized technical assistance center. Always use the same type of parts.
3. Maintenance and Installation

3.1  Maintenance
· To reduce the risk of electrical shock or fire, do not expose the power cable connector of this unit to rain or moisture.

· Intermittent usage will extend this fixtures service life.

· Please clear the fan, fan net, and optical lens of any dust or obstructions in order to keep the fixture in a proper working state.

· Do not use alcohol or any other organic solvent to wipe the shell.

3.2  Statement

All fixtures have been tested thoroughly before leaving the factory. In order to keep the product in good condition and ensure safe operation, users should follow the safety precautions and warnings in this manual.

   Important: Damages caused by not following the guidelines in this user manual are not covered under warranty. The manufacturer is not responsible for product issues caused by misuse.
3.3  Safety Precaution
· In order to guarantee the product’s life expectancy, do not store or use in environments over 60˚ C.
· Always mount this unit in a safe and stable manner. Mounting system must be able to withstand 10x that of the fixture’s weight. A safety cable must always be used as a secondary source for securing the fixture.

· Installation of this fixture may only be carried out by skilled individuals.
· This product can be used in the voltage range of 90-240V and is an indoor rated product. Please make sure that the power mains voltage used is not higher/or lower than what the product can withstand! The power plug must be inserted into a protected Class I socket and must be grounded properly. 
· In order to make sure the product is used properly, please read this manual carefully.
3.4  Cable connection (DMX)

   Make sure to use a cable conforming to specifications EIA RS-485: 2-pole twisted, shielded, 120Ohm characteristic impedance, 22-24 AWG, Low capacity. Do not use microphone cable or other cable with characteristics differing from those specified. The end connections must be made using XLR type 3-pin/ 5-pin male/female connectors. A terminating plug must be inserted into the last fixture with a resistance of 120 Ohm (minimum 1/4 W) between terminals 2 and 3.

IMPORTANT: The wires must not make contact with each other or with the metal casing of the connectors. The casing itself must be connected to the ground of the connector plugs.
4. Display Operation

The Fusion 7 FX comes equipped with a digital display screen which controls all the functions of the fixture. There are 4 control buttons also built-in for easier navigation through the display functions.

    4.1. Key Operation and Display instructions
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MENU：Function key
 UP：Plus   DOWN：Minus   ENTER：Confirm 
Menu List:
	No.
	Content
	Value
	Function instruction

	1
	A001
	001 - 512
	DMX512 Address setting 

	2
	33CH
	16/37
	Channel mode settings

	3
	U255
	000 - 255
	Main Amber color dimming, from dark to bright

	4
	R255
	000 - 255
	Auxiliary light red dimming, from dark to bright

	5
	G255
	000 - 255
	Auxiliary light green dimming, from dark to bright

	6
	B255
	000 - 255
	Auxiliary light blue dimming, from dark to bright

	7
	F000
	005 - 255
	Strobe

	8
	CL01
	01 - 20
	20 built-in color combinations to choose from

	9
	Au01
	01 - 10
	Auto effect，Press the Enter key to set the speed S000 - S255

	10
	Soud
	\
	Sound control，Press the Enter key to set the sensitivity to SE01 - SE15


Note: Manual menu function: Auto effect forward speed (0~127), reverse speed (128~255).

5. DMX Channel Charts

16 Channel Mode
	CH
	Value
	Description

	CH1
	000-255
	Total dimming

	CH2
	000-255
	Total strobe

	CH3
	000-255
	Main light dimming 1

	CH4
	000-255
	Main light dimming 2

	CH5
	000-255
	Main light dimming 3

	CH6
	000-255
	Main light dimming 4

	CH7
	000-255
	Main light dimming 5

	CH8
	000-255
	Main light dimming 6

	CH9
	000-255
	Main light dimming 7

	CH10
	000-255
	Auxiliary light red

	CH11
	000-255
	Auxiliary light green

	CH12
	000-255
	Auxiliary light blue

	CH13
	005-255
	Main color effect，See Appendix 1 for details

	CH14
	000-255
	Main color effect：Forward speed regulation 0-127，Reverse speed regulation 128-255；Sound control mode: Sound control sensitivity adjustment 0-255

	CH15
	000-255
	Auxiliary light effect，See Appendix 1 for details

	CH16
	000-255
	Auxiliary light effect forward speed adjustment 0-127，Reverse speed regulation 128-255；


37 Channel Mode
	CH
	Value
	Description

	CH1
	000-255
	Total dimming

	CH2
	000-255
	Total strobe

	CH3
	000-255
	Main light dimming 1

	CH4
	000-255
	Main light dimming 2

	CH5
	000-255
	Main light dimming 3

	CH6
	000-255
	Main light dimming 4

	CH7
	000-255
	Main light dimming 5

	CH8
	000-255
	Main light dimming 6

	CH9
	000-255
	Main light dimming 7

	CH10
	000-255
	Auxiliary light red

	CH11
	000-255
	Auxiliary light green

	CH12
	000-255
	Auxiliary light blue

	CH13
	005-255
	Main color effect，See Appendix 1 for details

	CH14
	000-255
	Main color effect：Forward speed regulation 0-127，Reverse speed regulation 128-255；Sound control mode: Sound control sensitivity adjustment 0-255

	CH15
	000-255
	Auxiliary light effect，See Appendix 1 for details

	CH16
	000-255
	Auxiliary light effect forward speed adjustment 0-127，Reverse speed regulation 128-255；

	CH17
	000-255
	Auxiliary light red 1

	CH18
	000-255
	Auxiliary light green 1

	CH19
	000-255
	Auxiliary light blue 1

	...
	...
	...

	...
	...
	...

	CH35
	000-255
	Auxiliary light red 7

	CH36
	000-255
	Auxiliary light green 7

	CH37
	000-255
	Auxiliary light blue 7


5.1 Appendix 1: Description of built-in effect functions
	CH13 Value
	Function
	CH15 Value
	Function

	0 - 4
	No effect
	0 - 4
	No effect

	5 - 11
12 - 18
19 - 25
26 - 32
33 - 39
40 - 46
47 - 53
54 - 60
61 - 67
68 - 74
75 - 81
82 - 88
89 - 95
96 - 102
103 - 109
110 - 116
117 - 123
124 - 130
131 - 137
138 - 144
145 - 151
152 - 158
159 - 165
166 - 172
173 - 179
180 - 186
187 - 193
194 - 200
201 - 207
208 - 214
	Mian light effect 1
Mian light effect 2
Mian light effect 3
Mian light effect 4
Mian light effect 5
Mian light effect 6
Mian light effect 7
Mian light effect 8
Mian light effect 9
Mian light effect 10
Mian light effect 11
Mian light effect 12
Mian light effect 13
Mian light effect 14
Mian light effect 15
Mian light effect 16
Mian light effect 17
Mian light effect 18
Mian light effect 19
Mian light effect 20
Mian light effect 21
Mian light effect 22
Mian light effect 23
Mian light effect 24
Mian light effect 25
Mian light effect 26
Mian light effect 27
Mian light effect 28
Mian light effect 29

Main light effect loop 30
	5 - 11
12 - 18
19 - 25
26 - 32
33 - 39
40 - 46
47 - 53
54 - 60
61 - 67
68 - 74
75 - 81
82 - 88
89 - 95
96 - 102
103 - 109
110 - 116
117 - 123
124 - 130
131 - 137
138 - 144
145 - 151
152 - 158
159 - 165
166 - 172
173 - 179
180 - 186
187 - 193
194 - 200
201 - 207
208 - 255
	Auxiliary light effect 1
Auxiliary light effect 2
Auxiliary light effect 3
Auxiliary light effect 4
Auxiliary light effect 5
Auxiliary light effect 6
Auxiliary light effect 7
Auxiliary light effect 8
Auxiliary light effect 9
Auxiliary light effect 10
Auxiliary light effect 11
Auxiliary light effect 12
Auxiliary light effect 13
Auxiliary light effect 14
Auxiliary light effect 15
Auxiliary light effect 16
Auxiliary light effect 17
Auxiliary light effect 18
Auxiliary light effect 19
Auxiliary light effect 20
Auxiliary light effect 21
Auxiliary light effect 22
Auxiliary light effect 23
Auxiliary light effect 24
Auxiliary light effect 25
Auxiliary light effect 26
Auxiliary light effect 27
Auxiliary light effect 28
Auxiliary light effect 29

Auxiliary light effect loop 30

	215 - 239
	Main light + auxiliary light effect
	
	

	240 - 244
	Sound effect 1
	
	

	245 - 249
	Sound effect 2
	
	

	250 - 255
	Sound effect 3
	
	


6. Technical Specifications
· Input voltage: AC100-240V/50-60Hz
· Max Power Draw: 400W

· Light Source: 7 x 50W Amber COB LEDs, 0.2W x SMD 5050 RGB LEDs
· Light Source Life: 50,000 hours

· Control Mode: DMX512, sound control, Auto, master-slave control

· DMX Input: 3-pin XLR head (XLR-3P)

· Channel Modes: 16/37 channels

· Strobe Speed: 0-20 times/second (speed adjustable)

· Protection Level: IP20

· Dimensions: 590*540*90mm / 23.3” x 21.3” x 3.5”
· Product Net Weight: 6.65 Kg / 14.7lb
7. Warranty

    This product carries a 1-year manufacturer’s warranty which covers factory defects or internal issues not caused by the owner/operator of the fixture. Misuse, physical damage, or any other issues caused by misuse by the customer are not covered under manufacturer’s warranty. All warranty claims must be handled directly through the manufacturer and not the dealer. Original sales receipt required for all warranty claims. Submit all claims to Info@Acueligthing.com.
For more information about this product as well as all our other products please visit:

www.AcueLighting.com

Or contact us directly:

Email: Info@AcueLighting.com
Phone: (818) 646-7526/ (818) 672-6822

