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1. INTRODUCTION
Thank you for choosing the Acue Magic Cube 9/16 IP. To use this product correctly and safely, please read the instructions carefully before installing and using this product. This manual contains important installation and operation information. Make sure to strictly follow the instructions when installing and operating this product. Retain this manual in a safe place for future reference. 

The Acue Magic Cube 9/16 IP uses a high-temperature resistant aluminum/metal body and is IP65 rated. IP65 is a classification given to devices that are designed mostly for outdoor use in various moist or wet environments. This product is designed and produced in strict accordance with CE standards and conforms to the international standard of DMX512 signal protocol. It can be controlled manually from the display or by DMX using the built in 3-pin XLR in/out connectors. This fixture is suitable for various types of indoor/outdoor concerts, indoor/outdoor events, indoor/outdoor installations, and other like environments.
2. SAFETY INSTRUCTIONS

· Please keep this User Manual for future reference. All users of this fixture must read the user manual thoroughly.

· Unpack and check contents carefully to make sure there is no damage caused by shipping before using the unit.

· Before operating, ensure that the voltage and frequency of power supply match the power requirements of the unit.

· It’s important to properly ground the fixture to avoid electric shock.

· The unit is designed for indoor/outdoor use. It is alright to use outdoors even when moisture is present. Do not point fixture directly into sunlight. Make sure main power connector is connected to an outlet that is not near liquids or moisture.
· The unit must be installed in a location with adequate ventilation, at least 50cm from adjacent surfaces. Be sure that no ventilation slots are blocked.

· Disconnect main power before moving fixture.

· Make sure there are no flammable materials close to the unit while operating, as it is fire hazard.

· Use safety cable when mounting this unit.
· Do not connect this product to power dimmers. 

· Max ambient operating temperature is 40˚ C. Do not operate if the temperature is higher than this.

· Unit surface temperature may reach up to 85˚ C. Do not touch the housing bare-handed during its operation. Turn off the power and allow about 15 minutes for the unit to cool down before replacing or serving.

· In the event of serious operating problem, stop using the unit immediately. Never try to repair the unit by yourself. Repairs carried out by unskilled individuals can lead to further damage or malfunction. Please contact the nearest authorized technical assistance center. Always use the same type of parts.
3. Maintenance and Installation

3.1  Maintenance
· To reduce the risk of electrical shock or fire, do not expose the power cable connector of this unit to rain or moisture.

· Intermittent usage will extend this fixtures service life.

· Please clear the fan, fan net, and optical lens of any dust or obstructions in order to keep the fixture in a proper working state.

· Do not use alcohol or any other organic solvent to wipe the shell.

3.2  Statement
All fixtures have been tested thoroughly before leaving the factory. In order to keep the product in good condition and ensure safe operation, users should follow the safety precautions and warnings in this manual.

   Important: Damages caused by not following the guidelines in this user manual are not covered under warranty. The manufacturer is not responsible for product issues caused by misuse.
3.3  Safety Precaution
· In order to guarantee the product’s life expectancy, do not store or use in environments over 60˚ C.
· Always mount this unit in a safe and stable manner. Mounting system must be able to withstand 10x that of the fixture’s weight. A safety cable must always be used as a secondary source for securing the fixture.

· Installation of this fixture may only be carried out by skilled individuals.
· This product can be used in the voltage range of 90-240V and is an indoor rated product. Please make sure that the power mains voltage used is not higher/or lower than what the product can withstand! The power plug must be inserted into a protected Class I socket and must be grounded properly. 
· In order to make sure the product is used properly, please read this manual carefully.
3.4  Cable connection (DMX)
   Make sure to use a cable conforming to specifications EIA RS-485: 2-pole twisted, shielded, 120 Ohm characteristic impedance, 22-24 AWG, Low capacity. Do not use microphone cable or other cable with characteristics differing from those specified. The end connections must be made using XLR type 3-pin/ 5-pin male/female connectors. A terminating plug must be inserted into the last fixture with a resistance of 120 Ohm (minimum 1/4 W) between terminals 2 and 3.
IMPORTANT: The wires must not make contact with each other or with the metal casing of the connectors. The casing itself must be connected to the ground of the connector plugs.
4. Display & Operation
The Magic Cube Par 9/16 IP fixtures are both equipped with IP65 rated LED displays with 4-button touch controls.
Menu Layout:

	Item
	Function
	Value
	Description

	DMX
	　DMX Address
	001-255
	DMX address code

	MANUAL
	Red
	000-255
	Dimming red

	
	Green
	000-255
	Dimming green

	
	Blue
	000-255
	Dimming blue

	
	Warm White
	000-255
	Dimming warm white

	
	Dimmer
	000-255
	Master dimmer

	
	Strobe
	000-255
	Strobe from slow to fast

	Auto
	Jump mode
	000-099
	Jump mode from slow to fast

	
	Fade mode
	000-099
	Fade mode from slow to fast

	
	Pulse mode
	000-099
	Pulse mode from slow to fast

	SETTING
	DMX Channel
	5CH/7CH/10CH
	DMX channel mode selection

	
	Display INV
	ON/OFF
	LCD display inverse

	
	Backlight
	OPEN/30/60
	Display background light

	
	Dimmer curve
	OFF/DIM1~4
	Dimming curve

	
	Key lock
	OFF/ON
	Lock button

	
	Default
	NO/YES
	Load default setting

	LANGUAGE
	Language
	English/Chinese
	System language

	INFO
	UID
	Unique ID
	　

	
	ADDR:
	　DMX address
	　

	
	VER:
	　Software version
	　

	
	Total time
	Total using time
	　

	
	Run time
	　Current using time
	　


5. DMX Connection & Charts
5.1 DMX Channel Chart
· 4 DMX Channel Mode

	CH
	VALUE
	FUNCTION

	1
	0-255
	Dimming red

	2
	0-255
	Dimming green

	3
	0-255
	Dimming blue

	4
	0-255
	Dimming warm white


· 6/9 DMX Channel Mode

	6CH
	9CH
	Function
	Value
	Description

	1
	1
	Dimmer
	000
	-
	255
	Master dimmer

	2
	2
	Strobe
	000
	-
	012
	Open

	
	
	
	013
	-
	255
	Strobe

	3
	3
	Dimmer
	000
	-
	255
	Dimming red

	4
	4
	
	000
	-
	255
	Dimming green

	5
	5
	
	000
	-
	255
	Dimming blue

	6
	6
	
	000
	-
	255
	Dimming warm white

	　
	7
	Static color
	000
	-
	031
	Off

	
	
	
	032
	-
	063
	Static red

	
	
	
	064
	-
	095
	Static green

	
	
	
	096
	-
	127
	Static blue

	
	
	
	128
	-
	159
	Static warm

	
	
	
	160
	-
	191
	Static red + green

	
	
	
	192
	-
	223
	Static red + blue

	
	
	
	224
	-
	255
	Static green + blue

	　
	8
	Macro function
	000
	-
	100
	Off

	
	
	
	101
	-
	150
	Jump mode

	
	
	
	151
	-
	200
	Fade mode

	
	
	
	201
	-
	255
	Pulse mode

	　
	9
	Macro Speed
	000
	-
	255
	Macro speed from slow to fast


5.2 DMX Connection
   The fixture is capable of receiving a DMX512 control signal. Connect the DMX controller to the fixture's DMX IN connector. Then, connect the fixture's DMX OUT connector to the DMX IN connector of the next fixture. Repeat this process for all additional fixtures in the DMX chain.
   For reliable signal transmission, it is recommended to install a DMX signal terminator at the end of the DMX chain. A terminator helps prevent signal interference caused by electrical noise and reflections.
A DMX terminator consists of a standard XLR connector with a 120 Ω resistor connected between Pin 2 and Pin 3. Insert the terminator into the DMX OUT connector of the last fixture in the chain, as shown in the illustration below.


6. Technical Specifications
	Model
	Magic Cube 9 IP
	Magic Cube 16 IP

	Power Supply
	AC100-240V/50-60Hz

	Max Power Consumption
	55W
	110W

	Light Source
	9pcs x 4in1 (RGB + Warm White)
	16pcs x 4in1 (RGB + Warm White)

	Lens Angle
	25°

	DMX Channel Modes
	4/6/9

	Control Mode
	DMX512, Auto, Master/Slave, RDM
	

	Display
	LCD + Touch button

	Working environment
	-15-35℃

	IP protection
	IP65 for indoor and outdoor use

	Packing size
	22x15x28Cm (1pc/CTN)

48x46x30Cm (6pcs/CTN)
	25x16x30Cm(1pc/CTN)

52x34.5x32Cm(4pcs/CTN)

	N.W.
	2.7Kg / 6lb
	3.5Kg / 7.75lb

	G.W.
	20.5Kg(6pcs/CTN) / 45lb
	17.6Kg / 39lb


7. Warranty

    This product carries a 1-year manufacturer’s warranty which covers factory defects or internal issues not caused by the owner/operator of the fixture. Misuse, physical damage, or any other issues caused by misuse by the customer are not covered under manufacturer’s warranty. All warranty claims must be handled directly through the manufacturer and not the dealer. Original sales receipt required for all warranty claims. Submit all claims to Info@Acueligthing.com.
For more information about this product as well as all our other products please visit:

www.AcueLighting.com

Or contact us directly:

Email: Info@AcueLighting.com
Phone: (818) 646-7526/ (818) 672-6822
PLEASE READ INSTRUCTIONS CAREFULLY BEFORE USE
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